**CAD V1 -> V2 Proposed Changes**

* Internal height 140mm -> ~160mm
* Additional exhausts on rear panel
* Plate thickness 15mm -> 12mm
* Consistent counterbores
* Tapped holes for cable routing
* Front panel extension
* Rear binding posts